{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["sheet1","sheet2","sheet3","sheet4","sheet5"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"sheet1","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[[22,2,25,2],[26,2,28,2],[1,3,4,3],[5,3,7,3],[8,3,11,3],[12,3,14,3],[15,3,18,3],[19,3,21,3],[22,3,25,3],[26,3,28,3],[1,2,4,2],[5,2,7,2],[8,2,11,2],[12,2,14,2],[15,2,18,2],[19,2,21,2],[8,4,11,4],[12,4,14,4],[15,4,18,4],[19,4,21,4],[22,4,25,4],[26,5,28,5],[29,5,32,5],[26,4,28,4],[29,4,32,4],[1,0,32,0],[1,5,4,5],[5,5,7,5],[8,5,11,5],[12,5,14,5],[15,5,18,5],[19,5,21,5],[22,5,25,5],[29,3,32,3],[29,2,32,2],[1,4,4,4],[5,4,7,4]]}
["TB. CUR.","TB. MARK","CABLE","CABLE NO.","TO DEVICE NAME","REMARK"]
["20A","U1","2.0MM*4C","AC1","NO1 ROLL PUMP AC440V 5HP","第一輪泵浦  AC440V 5HP"]
[null,"V1"]
[null,"W1"]
[null,"E"]
[null,"U2","2.0MM*4C","AC2","NO2 ROLL PUMP AC440V 5HP","第二輪泵浦 AC440V 5HP"]
[null,"V2"]
[null,"W2"]
[null,"U3","2.0MM*4C","AC3","NO3 ROLL PUMP AC440V 5HP","第三輪泵浦 AC440V 5HP"]
[null,"V3"]
[null,"W3"]
[null,"E"]
[null,"U4","2.0MM*4C","AC4","NO4 ROLL PUMP AC440V 5HP","第四輪泵浦 AC440V 5HP"]
[null,"V4"]
[null,"W4"]
[null,"U5","2.0MM*4C","AC5","A MIXING ROLL PUMP AC440V 5HP","A軋輪機泵浦 AC440V 5HP"]
[null,"V5"]
[null,"W5"]
[null,"E"]
[null,"U6","2.0MM*4C","AC6","B MIXING ROLL PUMP AC440V 5HP","B軋輪機泵浦 AC440V 5HP"]
[null,"V6"]
[null,"W6"]
[]
[]
[]
[]
[null,"U8","2.0MM*4C","AC8","TAKE-OFF ROLL PUMP AC440V 5HP","引出輪泵浦 AC440V 5HP"]
[null,"V8"]
[null,"W8"]

{"sheet":"sheet2","index":1,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,0,32,0],[1,2,4,2],[1,3,4,3],[1,4,4,4],[1,5,4,5],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[8,2,11,2],[8,3,11,3],[8,4,11,4],[8,5,11,5],[12,2,14,2],[12,3,14,3],[12,4,14,4],[12,5,14,5],[15,2,18,2],[15,3,18,3],[15,4,18,4],[15,5,18,5],[19,2,21,2],[19,3,21,3],[19,4,21,4],[19,5,21,5],[29,2,32,2],[29,3,32,3],[29,4,32,4],[29,5,32,5],[22,2,25,2],[22,3,25,3],[22,4,25,4],[22,5,25,5],[26,2,28,2],[26,3,28,3],[26,4,28,4],[26,5,28,5]]}
["TB. CUR.","TB. MARK","CABLE","CABLE NO.","TO DEVICE NAME","REMARK"]
["20A","U10","2.0MM*4C","AC10","NO1 ROLL PUMP FAN","第一輪泵浦風車 AC440V 2HP"]
[null,"V10"]
[null,"W10"]
[null,"E"]
[null,"U11","2.0MM*4C","AC11","NO2 ROLL PUMP FAN","第二輪泵浦風車 AC440V 2HP"]
[null,"V11"]
[null,"W11"]
[null,"U12","2.0MM*4C","AC12","NO3 ROLL PUMP FAN","第三輪泵浦風車 AC440V 2HP"]
[null,"V12"]
[null,"W12"]
[null,"E"]
[null,"U13","2.0MM*4C","AC13","NO4 ROLL PUMP FAN","第四輪泵浦風車 AC440V 2HP"]
[null,"V13"]
[null,"W13"]
[null,"U14","2.0MM*4C","AC14","A MIXING ROLL PUMP FAN","A軋輪機泵浦風車 AC440V 2HP"]
[null,"V14"]
[null,"W14"]
[null,"E"]
[null,"U15","2.0MM*4C","AC15","B MIXING ROLL PUMP FAN","B軋輪機泵浦風車 AC440V 2HP"]
[null,"V15"]
[null,"W15"]
[]
[]
[]
[]
[null,"U17","2.0MM*4C","AC17","TAKE-OFF ROLL PUMP FAN","引出輪泵浦風車 AC440V 2HP"]
[null,"V17"]
[null,"W17"]

{"sheet":"sheet3","index":2,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[[17,2,20,2],[17,3,20,3],[17,4,20,4],[1,2,4,2],[5,2,8,2],[9,2,12,2],[13,2,16,2],[1,3,4,3],[5,3,8,3],[9,3,12,3],[13,3,16,3],[29,4,32,4],[29,5,32,5],[1,4,4,4],[5,4,8,4],[9,4,12,4],[13,4,16,4],[1,0,32,0],[21,3,24,3],[21,4,24,4],[21,5,24,5],[25,2,28,2],[25,3,28,3],[25,4,28,4],[25,5,28,5],[1,5,4,5],[5,5,8,5],[9,5,12,5],[13,5,16,5],[17,5,20,5],[21,2,24,2],[29,2,32,2],[29,3,32,3]]}
["TB. CUR.","TB. MARK","CABLE","CABLE NO.","TO DEVICE NAME","REMARK"]
["10A","0607","1.25MM*4C","C1","NO1 ROLL 3 WIRES CONTROL VALVE","第一輪三線式電動閥"]
[null,"0608"]
[null,"T02"]
[]
[null,"A1","1.25MM*4C","C2","NO1 ROLL TEMPERATURE SENSOR","第一輪溫度感測器"]
[null,"B1"]
[null,"C1"]
[null,"SG"]
[null,"0617","1.25MM*4C","C3","NO2 ROLL 3 WIRES CONTROL VALVE","第二輪三線式電動閥"]
[null,"0618"]
[null,"T02"]
[]
[null,"A2","1.25MM*4C","C4","NO2 ROLL TEMPERATURE SENSOR","第二輪溫度感測器"]
[null,"B2"]
[null,"C2"]
[null,"SG"]
[null,"0707","1.25MM*4C","C5","NO3 ROLL 3 WIRES CONTROL VALVE","第三輪三線式電動閥"]
[null,"0708"]
[null,"T02"]
[]
[null,"A3","1.25MM*4C","C6","NO3 ROLL TEMPERATURE SENSOR","第三輪溫度感測器"]
[null,"B3"]
[null,"C3"]
[null,"SG"]
[null,"0717","1.25MM*4C","C7","NO4 ROLL 3 WIRES CONTROL VALVE","第四輪三線式電動閥"]
[null,"0718"]
[null,"T02"]
[]
[null,"A4","1.25MM*4C","C8","NO4 ROLL TEMPERATURE SENSOR","第四輪溫度感測器"]
[null,"B4"]
[null,"C4"]
[null,"SG"]

{"sheet":"sheet4","index":3,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,0,32,0],[1,2,4,2],[1,3,4,3],[1,4,4,4],[1,5,4,5],[5,2,8,2],[5,3,8,3],[5,4,8,4],[5,5,8,5],[9,2,12,2],[9,3,12,3],[9,4,12,4],[9,5,12,5],[13,2,16,2],[13,3,16,3],[13,4,16,4],[13,5,16,5],[17,2,20,2],[17,3,20,3],[17,4,20,4],[17,5,20,5],[29,2,32,2],[29,3,32,3],[29,4,32,4],[29,5,32,5],[21,2,24,2],[21,3,24,3],[21,4,24,4],[21,5,24,5],[25,2,28,2],[25,3,28,3],[25,4,28,4],[25,5,28,5]]}
["TB. CUR.","TB. MARK","CABLE","CABLE NO.","TO DEVICE NAME","REMARK"]
["10A","0807","1.25MM*4C","C9","A MIXING ROLL 3 WIRES CONTROL VALVE","A軋輪機三線式電動閥"]
[null,"0808"]
[null,"T02"]
[]
[null,"A5","1.25MM*4C","C10","A MIXING ROLL TEMPERATURE SENSOR","A軋輪機溫度感測器"]
[null,"B5"]
[null,"C5"]
[null,"SG"]
[null,"0817","1.25MM*4C","C11","B MIXING ROLL 3 WIRES CONTROL VALVE","B軋輪機三線式電動閥"]
[null,"0818"]
[null,"T02"]
[]
[null,"A6","1.25MM*4C","C12","B MIXING ROLL TEMPERATURE SENSOR","B軋輪機溫度感測器"]
[null,"B6"]
[null,"C6"]
[null,"SG"]
{"$rows_empty":8}
[null,"0917","1.25MM*4C","C15","TAKE-OFF ROLL 3 WIRES CONTROL VALVE","引出輪三線式電動閥"]
[null,"0918"]
[null,"T02"]
[]
[null,"A8","1.25MM*4C","C16","TAKE-OFF ROLL TEMPERATURE SENSOR","引出輪溫度感測器"]
[null,"B8"]
[null,"C8"]
[null,"SG"]

{"sheet":"sheet5","index":4,"n_rows":2,"n_cols":6,"rows_kept":2,"cut":false,"hidden":false,"merged":[[1,0,32,0],[1,2,4,2],[1,3,4,3],[1,4,4,4],[1,5,4,5],[5,2,8,2],[5,3,8,3],[5,4,8,4],[5,5,8,5],[9,2,12,2],[9,3,12,3],[9,4,12,4],[9,5,12,5],[13,2,16,2],[13,3,16,3],[13,4,16,4],[13,5,16,5],[17,2,20,2],[17,3,20,3],[17,4,20,4],[17,5,20,5],[29,2,32,2],[29,3,32,3],[29,4,32,4],[29,5,32,5],[21,2,24,2],[21,3,24,3],[21,4,24,4],[21,5,24,5],[25,2,28,2],[25,3,28,3],[25,4,28,4],[25,5,28,5]]}
["TB. CUR.","TB. MARK","CABLE","CABLE NO.","TO DEVICE NAME","REMARK"]
["10A"]